The project requires no special instructions other than to make sure the microcontroller is connected via USB to a computer and the code is uploaded. It is programmed with a 5 second calibration period during which one’s hand is placed over the photoresistor and slowly removed to allow the program to measure the ambient light.